Main routine

Move forward until one of the whiskers detect something

If hitleft()

Back up for 1 second

Turn right by powering right motor for 1 second

Resume moving forward

If hitright()  
 Back up for 1 second

Turn left by powering left motor for 1 second

Resume moving forward